Datasheet Board-to-Board 0.635mm (.025") Vertical Receptacle - Vertical Header 52760/52885:53475

[ Home > Products > Board-to-Board > Compare Products > Datasheet ] Help

PCB Orientation Parallel Pitch [mm (inches)] 0.635mm (.0250") Circuits 20, 30, 40, 50, 60, 68, 70, 80, 90, 100, 120, 140, 160, 180, 200, 240 Mated Height (H) 5.00mm (.197") Mated Width (W) 6.40mm (.252") Rows 2 Polarized to Mating Part Yes

Designed In Millimeters Temperature Range -55°C to +85°C Plating Contact Gold (Au) Current-max [amps] 0.5A Voltage-max [volts] 100V Contact Resistance [ohms] 40 milliohms max.

Withstanding Voltage 250V Insulation Resistance [ohms] 1000 Megohms min.

Receptacle - Orientation Vertical Receptacle - Mounting Surface Mount Receptacle - Locator Yes Receptacle - Polarized to PCB Yes

Receptacle - Stagger Tails No

Receptacle - Packaging Tube and embossed tape Receptacle - Housing Material LCP, Glass-filled, White

Receptacle - Flammability UL 94V-0 Receptacle - Contact Copper Alloy Header - Orientation Vertical Header - Mounting Surface Mount Header - Locator Yes Header - Polarized to PCB Yes

Header - Stagger Tails No Shrouded Yes Breakaway No Pin Header No

Female Receptacle 52760

Male Header 53475

Features and Benefits Sizes 20 to 240 circuits Anti-flux design Metal solder tabs provide pcb hold down and strain relief for SMT tails Polarizing pegs assist placement Receptacle:

Stacking height: 5.0mm, 6.0mm, 7.0mm, 8.0mm, 10.0mm Contact Resistance:40mW max. (H=5.0 to 7.0mm) 50mW max. (H=8.0, 10.0mm) Header:

Stacking height: 5.0mm,11.0mm Contact Resistance:40mW max. (H=5.0mm) 60mW max. (H=11.0mm)

Pin Header No Header - Packaging Tube and embossed tape Header - Housing Material PPS, Glass-filled, White Header - Flammability UL 94V-0 Header - Contact Copper Alloy

60mW max. (H=11.0mm)

[ © Copyright 2001 Molex Incorporated ]