Fotec Box 408, (A382-11 and A382-8), Measurement 1 (BWL 200MHz), Random Trigger

2

3

Figure 1: Occupancy versus threshold voltage. Left for measuremnt m1 r2 F408, right for this measuremnt. Legende: signal labels the plot where the time window was around the signal while for noise graphs the time window was set at the begining of the waveform.

Data File = SP 060403121914 Fotec408-A382-11-A382-8 measurement1 RandomTrigg.xls Upper Diamond = A382-11 Lower Diamond = A382-8 Maček ceramic Ass. #1 Resistor still 130Ω.

Setup the same as with normal HV scans, only fotec box was placed away from the source (^{90}Sr).