Fotec Box 408, (A382-11 and A382-8), Measurement 1 (BWL 200MHz), resistor changed 150Ω → 130Ω

2

3

4

Data File = SP 060322170035 Fotec408 A382-11 A382-8 measurement1.xls Upper Diamond = A382-11 Lower Diamond = A382-8 Maček ceramic Ass. #1 resistor (marked with green circle on Fig.1) changed: 150Ω → 130Ω

Figure 1: BCM schematics.