Fotec Box 408, (A382-11 and A382-8), Measurement 1 (BWL 200MHz)

2

3

4

Data File = /SP 060329154405 Fotec408 A382-11 A382-8 NoMagnet-vertical.xls Upper Diamond = A382-11 Lower Diamond = A382-8 Maček ceramic Ass. #1 Magnetic field was turned off before the measurement started. Setup stayed the same as with measurement SP 060328175027 Fotec408 A382-11 A382-8 Magnet-vertical.xls, where the magnetic filed was on.