I. Mandic SCT week 31.1.-4. 2. 2000 2

Oslo Hybrid with 6 ABCD2T chips was irradiated in the reactor in Ljubljana

This hybrid was irradiated to 1.5 x 10^{14}n/cm^2 in November another irradiation with 0.5 x 10^{14}n/cm^2was done to get the total fluence of 2 x 10^{14}n/cm^2

� threshold scans were done: - edge detect, edge (01X) data compression - pulses 1.5, 2.0 and 2.5 fC - at different preamplifier and shaper bias currents settings